SRS components are located in this area. Review the SRS component locations LHD, SRS component locations RHD and the precautions and procedures before performing repairs or service. NOTE:

- Use the handy remover set, or equivalent when prying components.
- Take care not to bend or scratch the headliner.
- Be careful not to damage the dashboard and other interior trim.

1. Remove these items:
   - Front pillar trim, both sides, without side curtain airbag, with side curtain airbag
   - Ceiling light
   - Front seat belt upper anchor, both sides
   - Center pillar lower trim, without side curtain airbags, with side curtain airbags
   - Center pillar upper trim, both sides, without side curtain airbags, with side curtain airbags
   - Rear pillar trim, both sides, without side curtain airbags, with side curtain airbags

1. From both sides, using a flat-tip screwdriver, release the tabs (A), then remove the sunvisor cap (B) from the bracket (C). Turn the cap, and remove it.