1. Measure the voltage between the No. 3 terminal of the A/C condenser fan relay 4P socket and body ground.

Is there battery voltage?

YES | - | Go to Step 8 .
NO | - | Repair open in the wire between the No. 30 fuse in the under-dash fuse/relay box and the A/C condenser fan relay.■

1. Turn the ignition switch OFF.

1. Reinstall the A/C condenser fan relay.

1. Remove A/C diode A from the left side (LHD) or the right side (RHD) of the dashboard.