Maintenance Schedule for Normal and Severe Conditions - Except EU

This Maintenance Schedule outlines the minimum required maintenance that you should perform to ensure the trouble-free operation of the vehicle. Due to regional and climatic differences, some additional service may be required. Please consult the warranty booklet for a more detalied description.
The following items must be used for ‘‘severe conditions'' indicated on schedule, if the vehicle is driven MAINLY under the specified conditions A to E.

- Engine oil and engine oil filter: A/B/C/D/E
- Air cleaner element: D/E
- Transmission fluid: B/D

A: Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
B: Driving in extremely hot over 35 °C (95 °F) conditions.
C: Extensive idling, or long periods of stop-and-go driving.
D: Trailer towing, driving with a loaded roof rack, or driving in mountainous conditions.
E: Driving on muddy, dusty, or de-iced roads.

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Replace engine oil and filter | Normal conditions | Every 10,000 km (6,250 miles) or 1 year
Severe conditions | Every 5,000 km (3,125 miles) or 6 months
Replace air cleaner element | Normal conditions | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Severe conditions | Every 10,000 km (6,250 miles)
Replace fuel filter Replace fuel filter every 40,000 km (25,000 miles) or 2 years, if the fuel the customer uses is suspected to be contaminated. | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Inspect drive belt Look for cracks and damage, then check the position of the drive belt auto-tensioner indicator. |  | ● |  | ● |  | ● |  | ● |  | ●
Replace engine coolant Use genuine Honda All Season Antifreeze/Coolant Type 2. |  |  |  |  | ● |  |  | ● |  |
Replace Manual Transmission Fluid (MTF) Use genuine Honda MTF. | Normal Conditions |  |  |  |  |  | ● |  |  |  |
Severe Conditions |  |  | ● |  |  | ● |  |  | ● |

Service at the indicated distance or time whichever comes first | km x 1,000 | 20 | 40 | 60 | 80 | 100 | 120 | 140 | 160 | 180 | 200
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
miles x 1,000 | 12.5 | 25.0 | 37.5 | 50.0 | 62.5 | 75.0 | 87.5 | 100.0 | 112.5 | 125.0
months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96 | 108 | 120
Check front and rear brakes Check the brake pad and disc thickness. Check for damage or cracks. | Every 10,000 km (6,250 miles) or 6 months
Replace brake fluid

- Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid.
- Check the brake fluid level is between the upper and lower marks on the reservoir.

Every 3 years
Check parking brake adjustment Check the parking brake operation. | ● | ● |  | ● |  | ● |  | ● |  | ●
Replace dust and pollen filter | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
Rotate tyres Check tyre inflation at least once per month. | Every 10,000 km (6,250 miles)

Visually inspect the following items:
- Check for correct installation and position, check for cracks, deterioration, rust, and leaks.
- Check tightness of screws, nuts, and joints. If necessary, retighten.

Tie-rod ends, steering gearbox, and boots

- Check rack grease and steering linkage.
- Check the boot for damage and leaking grease.

Every 10,000 km (6,250 miles) or 6 months
Suspension components

- Check the bolts for tightness.
- Check all dust covers for deterioration and damage.

Driveshaft boots

- Check the boot and boot band for cracks.
- Check rack grease.

Brake hoses and lines (including VSA lines) Check the master cylinder and VSA modulator-control unit and leakage. | ● | ● | ● | ● | ● | ● | ● | ● | ● | ●
All fluid levels and condition of fluid Check levels and check for leaks. If necessary, add.

- Engine coolant
- MTF
- Clutch fluid
- Power steering fluid
- Brake fluid
- Windshield fluid

Exhaust system Check the catalytic converter heat shield, exhaust pipe, and muffler for damage, leaks, and tightness.
Fuel lines and connections

- Check fuel lines for loose connections, cracks, and deterioration.
- Retighten loose connections and replace any damaged parts.