1. If necessary, remove the screws, then remove the upper grille molding (A), lower grille molding (B), center grille molding (C), center grille base (D), emblem (E), emblem base (F), air guide grille (G), front grille molding (H), from the front grille cover (I).

1. Install the front grille in the reverse order of removal, and check the clips for damage or stress-whitening, and if necessary, replace them with new ones.

With adaptive cruise control
Without adaptive cruise control
Type-S