Intermediate Shaft Disassembly

Special Tools Required Oil seal driver 07947-SB00100 Half shaft base 07NAF-SR30101

1. Remove the set ring (A), outer seal (B), and external snap ring (C).

1. Press the intermediate shaft (A) out of the intermediate shaft bearing (B) using a press. Be careful not to damage the metal rings (C) on the intermediate shaft during disassembly.

1. Remove the internal snap ring.

1. Press the intermediate shaft bearing (A) out of the bearing support (B) using the special tools and a press.