NOTE:

- Do not use this troubleshooting procedure if the radiator fan and/or the A/C compressor is inoperative. Refer to the symptom troubleshooting index.
- Before performing symptom troubleshooting, check for powertrain DTCs.

1. Check the No. 30 (7.5 A) fuse in the under-dash fuse/relay box.

Is the fuse OK?

YES | - | Go to Step 2 .
NO | - | Replace the fuse, and recheck.■

1. Remove the fan control relay from the multi-relay box, and test it.

Is the relay OK?

YES | - | Go to Step 3 .
NO | - | Replace the fan control relay.■

1. Turn the ignition switch ON (II).

1. Measure the voltage between the No. 5 terminal of the fan control relay 5P socket and body ground.

Is there battery voltage?

YES | - | Go to Step 5 .
NO | - | Go to Step 17 .

1. Turn the ignition switch OFF.