Taillight Replacement

Taillight

1. Remove the rear bumper.

1. Open the trunk lid and remove the trunk side trim panel.

1. Disconnect the connectors (A) from the taillight (B).

   Brake/Taillight: | 21/5 W
   Turn signal Light: | 21 W

1. Remove the mounting nuts and screws, then remove the taillight.

1. Turn the bulb socket 45 ° counterclockwise to remove the bulb.

1. Inspect the gasket; replace it if it is distorted or stays compressed.

1. Install the taillight and tighten the nuts to 5 N·m (0.5 kgf·m, 4 lbf·ft).

1. After installing the taillight, run water over it to make sure it does not leak.

Inner Taillight

1. Open the trunk lid and disconnect the connectors (A) from the trunk lid.

   Taillight: | 5 W
   Back-up Light: | 21 W
   Rear Fog Light: | 21 W

1. Remove the three nuts and the inner taillight (B).

1. Turn the bulb socket 45 ° counterclockwise to remove the bulb.

1. Inspect the gasket; replace it if it is distorted or stays compressed.

1. Install the taillight and tighten the nuts to 5 N·m (0.5 kgf·m, 4 lbf·ft).

1. After installing the taillight, run water over it to make sure it does not leak.