1. Check for continuity between the VSA control unit 47P connector terminal No. 25 and sensor cluster 6P connector terminal No. 3.

Is there continuity?

YES | - | Go to Step 16 .
NO | - | Repair open in the wire between the VSA modulator-control unit and the sensor cluster.■

1. Substitute a known-good sensor cluster.

1. Reconnect all of the disconnected connectors.

1. Clear the DTC using the HDS.

1. Disconnect the HDS from the 16P DLC.

1. Turn the ignition switch OFF, then turn it ON (II) again.

1. Test-drive the vehicle around a number of corners.

1. Verify the DTC.

Is DTC 25 indicated?

YES | - | Replace the VSA modulator-control unit. ■
NO | - | Replace the original sensor cluster. ■