1. Aim the light toward the pointer (A) on the cam chain case. Check the ignition timing under a no load condition (headlights, blower fan, rear window defogger, and air conditioner are turned off).

   Ignition Timing
   M/T: | 8 ° ± 2 ° BTDC (RED mark (B)) at idle in Neutral
   A/T: | 8 ° ± 2 ° BTDC (RED mark (B)) at idle in Park or Neutral

1. If the ignition timing differs from the specification, check the cam timing. If the cam timing is OK, update the engine control module (ECM)/powertrain control module (PCM) if it does not have the latest software, or substitute a known-good ECM/PCM, then recheck. If the system works properly, and the ECM/PCM was substituted, replace the original ECM/PCM.

1. Disconnect the HDS and the timing light.

1. Secure the service loop to the wire harness with wire ties.