1. Release the clips (A) from middle and rear of the carpet (B), and pull back the rear floor carpet (C).

1. Release the hooks (D) with a flat-tip screwdriver by pushing the screwdriver toward the door, then lift upwards. Pull the fastener (E) out, then remove the carpet.

1. Install the carpet in the reverse order of removal, and note these items:
   - Take care not to damage, wrinkle or twist the carpet.
   - Make sure the seat harnesses and antenna lead are routed correctly.
   - Replace any damaged clips.
   - Reconnect the negative cable to the battery.
   - Reset the clock.
   - Perform the power window control unit reset procedure.