1. Check for continuity between LKAS control unit 26P connector terminal No. 25 and gauge control module connector (36P) terminal No. 19.

Is there continuity?

YES | - | Check for loose terminals in the gauge control module connector, and repair if necessary. If no poor connections are found, replace the gauge control module. ■
NO | - | Repair an open in the wire between the LKAS control unit and the branch of the F-CAN (CANL).■