Exploded View Special Tools Required Driver, 40 mm I.D. 07746-0030100 Driver, 30 mm I.D.
07946-MB00000
NOTE: Refer to the Exploded View as needed during this procedure.

1. Clean all parts in solvent, dry them, and apply lubricant to all contact surfaces except the 3rd/4th and 5th synchro hubs.

1. Install the new angular ball bearing (A) using the special tool and a press. Note the direction of installation.