Clutch Pedal Position Switch Test

Clutch Pedal Position Switch A

1. Disconnect the clutch pedal position switch A 2P connector.

1. Remove the clutch pedal position switch A.

1. Check for continuity between the terminals according to the table.
   - If the continuity is not as specified, replace the clutch pedal position switch A.
   - If OK, install clutch pedal position switch A and adjust the pedal height.

Clutch Pedal Position Switch B

1. Disconnect the clutch pedal position switch B 3P connector.

1. Remove the clutch pedal position switch B.

1. Check for continuity between the terminals according to the table.
   - If the continuity is not as specified, replace the clutch pedal position switch B.
   - If OK, install clutch pedal position switch B and adjust the pedal height.