Stereo Amplifier Connector Replacement

When replacing the stereo amplifier connector, match the wires to the cavities listed in the following table.

Cavity | Wire | Connect to | Cavity | Wire | Connect to
--- | --- | --- | --- | --- | ---
A1 | BLK/RED | Right tweeter (+) | A11 | PNK/BLK | Right tweeter (−)
A2 | GRN/YEL | Front passenger's door speaker (+) | A12 | GRY | Front passenger's door speaker (−)
A3 | GRN/BLK | Driver's door speaker (+) | A13 | LT GRN | Driver's door speaker (−)
A4 | BLU/ORN | Left tweeter (+) | A14 | GRY/BLU | Left tweeter (−)
A5 | RED | Right rear speaker (+) | A15 | BRN | Right rear speaker (−)
A6 | WHT | Left rear speaker (+) | A16 | GRN | Left rear speaker (−)
A7 | BLU/RED | Right rear door speaker (+) | A17 | BLU/ORN | Right rear door speaker (−)
A8 | PNK/BLU | Left rear door speaker (+) | A18 | PUR | Left rear door speaker (−)
A9 | RED | ACC (main stereo power supply) | A19 | ——— | Not used
A10 | WHT/BLU | Constant power | A20 | BLK | Ground (G504)
B1 | RED/BLU | Audio unit (Driver's door speaker (+)) | B8 | YEL | Audio unit (Driver's door speaker (−))
B2 | BRN/YEL | Front passenger's shielding | B9 | GRY/BLU | Left rear shielding
B3 | BLU | Audio unit (Left rear speaker (+)) | B10 | PNK | Audio unit (Left rear speaker (−))
B4 | BLU | Audio unit (Front passenger's door speaker (+)) | B11 | RED | Audio unit (Front passenger's door speaker (−))
B5 | BRN | Driver's shielding | B12 | GRY | Right rear shielding
B6 | LT GRN | Audio unit (Right rear speaker (+)) | B13 | PUR | Audio unit (Right rear speaker (−))
B7 | YEL/GRN | Audio unit (Radio switch) | B14 | BLK | Ground (G504)

With Premium Audio