1. Install the shift solenoid harness connector (F) in the transmission housing with the new O-ring (G).

1. Connect the connector (YEL, WHT, and WHT wires) to the shift solenoid valve D.

1. Connect the connectors to the respective valves:
   - BLU wire to shift solenoid valve A.
   - ORN wire to shift solenoid valve B.
   - GRN wire to shift solenoid valve C.
   - RED wire to shift solenoid valve E.