1. Remove the side engine mount bracket.

1. Check that the engine/transmission is completely free of vacuum hoses, fuel and coolant hoses, and electrical wiring.

1. Slowly raise the engine/transmission assembly about 150 mm (6 in.). Check once again that all hoses and wires are disconnected from the engine/transmission.

1. Raise the engine/transmission assembly all the way, and remove it from the vehicle.