Fuel Filter Removal/Installation

Special Tools Required Fuel filter wrench 070AA-RMAC100

1. Remove the hand primer.

1. Remove the air cleaner.

1. Disconnect the connectors and the hand clips.

1. Remove the bolts (A).

1. Remove the fuel filter bracket (B).

1. Set the fuel filter (A) to the vice. Attach the fual filter wrench assy.

1. Remove the fuel filter water level switch.

1. Remove the fuel filter.

1. Install the part in the reverse order of removal with a new O-ring (B).

1. Bleed the fuel system.