1. With a sponge, carefully apply a light coat of body primer to any exposed paint or metal around the flange where new adhesive will be applied. Let the primer dry for at least 10 minutes:
   - Do NOT apply body primer to any remaining original adhesive on the flange.
   - Be careful not to mix up the body and glass primer sponges.
   - Never touch the primed surfaces with your hands.
   - Use a body line (A) in the upside and both sides of the rear window opening flange as a guide to keep within width of the body primer shown while applying.