1. Disconnect the wire harness connectors from the combination switch assembly (A).

1. Remove the combination switch assembly from the steering column shaft by removing the screws (B).

1. Disconnect the connectors from the ignition switch, and release the wire harness clips from the steering column.

1. Remove the steering joint bolt (C), then disconnect the steering joint (D) from the pinion shaft.

1. Remove the steering column (E) by removing the attaching nuts and bolts. If the lower slide shaft (F) is removed, slip it into the upper shaft (G) by aligning the paint or stamped marks (H).