Removal

1. Disconnect the negative battery cable, and wait at least 3 minutes before beginning work.

1. Disconnect the driver's airbag 2P connector, the front passenger's airbag 2P connector, both seat belt tensioner 4P connectors.

1. Remove the front inner fender.

1. Disconnect the engine compartment wire harness 2P connector (A), and remove the two Torx bolts (B) using a Torx T30 bit, then remove the front impact sensor (C).