Retainer Replacement

1. Gradually scrape off the adhesive tape (A) under the retainers (B) while heating it with a heat gun.
   NOTE:
   - Avoid overheating the painted surfaces around the retainers.
   - Wrap the exterior resin parts near the front pillar with aluminum foil to protect them from overheating.

1. Clean the body bonding surface with a sponge dampened in alcohol. After cleaning, keep oil, grease, and water from getting on the surface.