1. Install the pulley (A), then loosely install the pulley nut (B). Hold the steering pump in a vise with soft jaws (C). Be careful not to damage the pump housing with the jaws of the vise.

1. Hold the pulley with the special tool, and tighten the pulley nut to the specified torque.

1. Check that the pump turns smoothly by turning the pulley. If it turns hard, loosen the four flange bolts on the cover, then retightening them in the same manner as in the Step 35 . Turning the pump again by hand.