1. Install the stabilizer link (A) on the stabilizer bar (B) and lower arm (C) with the joint pins set at the center of their range of the movement.
   NOTE: The left stabilizer link has a yellow paint mark (D), while the right stabilizer link has a white paint mark.

1. Install a new self-locking nut and flange nut, and lightly tighten them.
   NOTE: Use a new self-locking nut on reassembly.

1. Place the floor jack under the lower arm, and raise the suspension to load it with the vehicle's weight.
   Do not place the jack against the ball joint pin of the knuckle.