NOTE:

- Do not use this troubleshooting procedure if the A/C compressor is inoperative. Refer to the symptom troubleshooting index.
- Before performing symptom troubleshooting, check for powertrain DTCs.

1. Check the No. 9 (20 A) fuse in the under-hood fuse/relay box, and the No. 30 (7.5 A) fuse in the under-dash fuse/relay box.

Are the fuses OK?

YES | - | Go to Step 2 .
NO | - | Replace the fuse(s), and recheck.■

1. Remove the A/C condenser fan relay from the under-hood fuse/relay box, and test it.

Is the relay OK?

YES | - | Go to Step 3 .
NO | - | Replace the A/C condenser fan relay .■

1. Measure the voltage between the No. 1 terminal of the A/C condenser fan relay 4P socket and body ground.

Is there battery voltage?

YES | - | Go to Step 4 .
NO | - | Replace the under-hood fuse/relay box.■