Rear Door Sill Area NOTE:

- Put on gloves to protect your hands.
- Take care not to bend or scratch the trim and panels.
- Use the handy remover set, or equivalent when prying components.

1. Detach the hook (A) and tab (B) from the center pillar lower trim (C), and pull the rear door sill trim (D) up by hand to detach the clips (E, F), then remove it.

1. If necessary, pull the rear side outer trim (G) up to detach the clips (H), then remove the trim.