1. Reassemble the rocker arm assembly.

1. Clean and dry the No. 5 rocker shaft holder mating surface.

1. Apply liquid gasket, P/N 08C70-K0234M, 08C70-K0334M, or 08C70-X0331S, evenly to the cylinder head mating surface of the No. 5 rocker shaft holder.
   NOTE: Do not install the parts if 4 minutes or more have elapsed since applying liquid gasket. Instead, reapply liquid gasket after removing old residue.