Radiator and Fan Replacement

1. Drain the engine coolant.

1. Remove the lower radiator hose from the radiator.

1. A/T model: Remove the automatic transmission fluid (ATF) cooler hoses.

1. Remove the upper radiator hose and lower radiator hose from the radiator.

1. Disconnect the fan motor connectors and radiator fan switch connector.

1. Remove the upper bracket cushions, then pull up the radiator.

1. Remove the fan shroud assemblies and other parts from the radiator.

1. Install the radiator in the reverse order of removal. Make sure the upper and lower cushions are set securely.

1. Fill the radiator with engine coolant and bleed the air.