A/T Differential Carrier Bearing Outer Race Replacement

Special Tools Required Handle driver 07749-0010000 Driver attachment, 78 x 90 mm 07GAD-SD40101
Driver attachment, 72 x 75 mm
07746-0010600
NOTE:

- The bearing and bearing outer race should be replaced as a set.
- Replace the bearing with a new one whenever the outer race is replaced.
- Do not use the thrust shim on the torque converter housing.
- Adjust bearing preload after replacing the bearing and outer race.
- Coat all parts with ATF during installation.

1. Remove the bearing outer race (A), 76.2 mm thrust washer (B), and 76 mm thrust shim (C) from the transmission housing (D) by heating the housing to about 100 °C (212 °F) with a heat gun (E). Do not heat the housing more than 100 °C (212 °F).
   NOTE: Let the transmission housing cool to room temperature before installing the bearing outer race.

1. Remove the bearing outer race (A) and 80 mm thrust washer (B) from the torque converter housing (C).

1. Install the 80 mm thrust washer and the new bearing outer race in the torque converter housing.

1. Install the bearing outer race securely in the torque converter housing with the handle driver and 78 x 90 mm driver attachment.

1. Install the 76 mm thrust shim (A), 76.2 mm thrust washer (B), and the new bearing outer race (C) in the transmission housing (D).
   NOTE: Install the 76.2 mm thrust washer with the ‘‘41382RKY'' mark facing downward.

1. Install the bearing outer race securely so there is no clearance between the outer race, thrust washer, thrust shim and the transmission housing with the handle driver and 72 x 75 mm driver attachment.