Target pattern surface height adjustment

1. Move the radar aimer set to the front of the vehicle so that the target pattern faces the vehicle.

1. Measure and adjust the height between the center of the target pattern of the radar aimer set to the specified height value Z.

   LKAS camera height setting value number | Prescribed distance X (mm)
   1,500 | 2,000 | 2,500 | 3,000
   (1) | 1,178 | 1,152 | 1,126 | 1,100
   (2) | 1,174 | 1,149 | 1,125 | 1,100
   (3) | 1,170 | 1,147 | 1,123 | 1,100
   (4) | 1,166 | 1,144 | 1,122 | 1,100
   (5) | 1,163 | 1,142 | 1,121 | 1,100

   NOTE:
   - The specified height value Z is different according to the prescribed distance X described in Step 3 and the camera height setting value described in Step 20 . Choose and use the height value Z which corresponds to the selected distance and the camera height setting number.
   - Measure the height precisely using a scale. Do not use the height graduation on the radar aimer set as a guide.