1. Install the drive belt (A).
   Note these items during belt installation:
   - Make sure that the belt is properly positioned on the pulleys (B).
   - Do not get power steering fluid or grease on the auto-tensioner, alternator, A/C compressor, drive belt, or pulley faces. Clean off any fluid or grease before installation.

1. Tighten the pump mounting bolts to the specified torque.

1. Fill the reservoir to the upper level line.