ECM/PCM Inputs and Outputs at Connector A (31P)
NOTE: Standard battery voltage is 12 V.

Terminal number | Wire color | Terminal name | Description | Signal
--- | --- | --- | --- | ---
20 | YEL/BLU | VCC2 (SENSOR VOLTAGE) | Provides sensor voltage | With ignition switch ON (II): about 5 V With ignition switch OFF: about 0 V
21 | YEL/RED | VCC1 (SENSOR VOLTAGE) | Provides sensor voltage | With ignition switch ON (II): about 5 V With ignition switch OFF: about 0 V
23 | GRN/YEL | SG2 (SENSOR GROUND) | Sensor ground | Less than 1.0 V at all times
24 | GRN/WHT | SG1 (SENSOR GROUND) | Sensor ground | Less than 1.0 V at all times
25 *2 | RED/YEL | APSB (ACCELERATOR PEDAL POSITION (APP) SENSOR B) | Detects APP sensor B signal | With ignition switch ON (II) and accelerator pedal pressed: about 2.3 V With ignition switch ON (II) and accelerator pedal released: about 0.2 V
26 *2 | RED/BLU | APSA (ACCELERATOR PEDAL POSITION (APP) SENSOR A) | Detects APP sensor A signal | With ignition switch ON (II) and accelerator pedal pressed: about 4.5 V With ignition switch ON (II) and accelerator pedal released: about 0.5 V
28 | RED/YEL | AFS− (AIR FUEL RATIO (A/F) SENSOR, SENSOR 1 −SIDE) | Detects A/F sensor (sensor 1) signal |
29 *1 | RED/BLK | TPS (THROTTLE POSITION SENSOR) | Detects TP sensor signal | With throttle fully open: about 4.5 V typically With throttle fully closed: about 0.5 V
30 | GRN/RED | MAP (MANIFOLD ABSOLUTE PRESSURE SENSOR) | Detects MAP sensor signal | With ignition switch ON (II): about 3V At idle: about 1.0 V (depending on engine speed)
31 | RED | AFS+ (AIR FUEL RATIO (A/F) SENSOR, SENSOR 1 +SIDE) | Detects A/F sensor (sensor 1) signal |

*1: | K20A6 engine
*2: | K24A3 engine