Rear Camber Inspection

1. Raise the rear of the vehicle, and remove the wheel caps.
   NOTE: Push out the cap on the aluminum wheel from the inside after removing the wheel.

1. Install the wheel alignment gauge attachment (A) and camber/caster gauge on the wheel hub.

1. Read the camber angle on the gauge with the bubble at the center of the gauge. If the camber angle is not within the specification, check for bent or damaged suspension components.

   Rear camber angle: | −1 ° 00 '±30 '