Transmission Mount Bracket Removal/Installation - Upper

1. Support the engine with a jack and wood block under the transmission.

1. Remove the air cleaner housing.

1. Remove the transmission upper mount bracket (A).

1. Install the transmission upper mount bracket, and tighten the new bolts, then loosely tighten the mounting bolt (B).

1. Remove a jack.

1. Loosen the transmission upper mount mounting bolt/nuts (A), then retighten the mounting bolt/nuts.

1. Tighten the transmission upper mount bracket mounting bolt (B).

1. Install the air cleaner housing.