Cylinder Head Rocker Arm and Shaft Disassembly/Reassembly

NOTE:

- Identify parts as they are removed to ensure reinstallation in original location.
- Inspect the rocker arm shaft and rocker arms.
- The rocker arms must be installed in the same positions if reused.
- When removing or installing the rocker arm assembly, do not remove the camshaft holder bolts. The bolts will keep the holders and rocker arms on the shaft.
- Prior to reassembling, clean all the parts in solvent, dry them, and apply lubricant to any contact points.
- Bundle the intake rocker arms with rubber bands to keep them together as a set.
- When replacing the VTEC rocker arm assembly, remove the fastening hardware from the new VTEC rocker arm assembly.

K20A6 engine:
K24A3 engine: