1. Attach the fasteners (A) with adhesive tape and rubber dam (B) to the inside face of the rear window (C) as shown. Attach the molding (D) with adhesive tape along the edge of the rear window. Before installing the molding, apply primer to the inside face of the rear window.
   - Be sure the fasteners and upper rubber dam line up with alignment marks (E).
   - Be careful not to touch the rear window where adhesive will be applied.

   Fasteners adhesive tape:
   | Thickness 0.6 mm (0.02 in.) Width 7.5 mm (0.3 in.)
   Rubber dam adhesive tape:
   | Thickness 0.16 mm (0.0063 in.) Width 3 mm (0.1 in.)
   Molding adhesive tape:
   | Thickness 0.2 mm (0.008 in.) Width 4 mm (0.16 in.)