M/T Reverse Shift Fork Clearance Inspection

1. Measure the clearance between the reverse idler gear (A) and the reverse shift fork (B) with a feeler gauge (C). If the clearance is more than the service limit, go to Step 2 .

   Standard: | 0.20−0.59 mm (0.007−0.024 in.)
   Service Limit: | 1.2 mm (0.047 in.)

1. Measure the width of the reverse shift fork.
   - If distance is not within the standard, replace the reverse shift fork with a new one.
   - If distance is within the standard, replace the reverse gear with a new one.

   Standard: | 13.4−13.7 mm (0.527−0.539 in.)