1. To remove a rear drain valve (A) from the body, remove these parts:
   - Spare tyre lid

   - | Without trunk side spacer
   - | With trunk side spacer

   - Trunk side spacer, if equipped
   - Trunk rear trim panel

   - | Without trunk side spacer
   - | With trunk side spacer

   Tie a string to the top end of the rear drain tube (B), then pull back the trunk side trim panel and pull the drain tube down out of the pillar leaving the string inside the pillar.