1. Loosen the pressure bolt (A), and install the special tool as shown. Insert the jaws carefully, making sure not to damage the ball joint boot. Adjust the jaw spacing by turning the adjusting bolt (B).
   NOTE: For using 07MAC-SL00201, fasten the safety tie (C) securely to a suspension arm or the subframe (D). Do not fasten it to a brake line or wire harness.

1. After adjusting the adjusting bolt, make sure the head (E) of the adjusting bolt is in the position shown to allow the jaw to pivot.

1. With a wrench, tighten the pressure bolt until the ball joint pin pops loose from the ball joint pin hole. If necessary, apply penetrating type lubricant to loosen the ball joint pin.
   NOTE: Do not use pneumatic or electric tools on the pressure bolt.

1. Remove the tool, then remove the nut from the end of the ball joint pin, and pull the ball joint out of the ball joint pin hole. Inspect the ball joint boot, and replace it if damaged.