DTC P2017: IMRC Valve Position Sensor Circuit High Voltage

1. Turn the ignition switch ON (II).

1. Check the IMRC VALVE POSITION SENSOR in the DATA LIST with the HDS.

Is about 4.90 V or higher indicated?

YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the IMRC valve position sensor and the ECM.■

1. Turn the ignition switch OFF.

1. Disconnect the IMRC valve position sensor 3P connector.

1. Connect IMRC valve position sensor 3P connector terminals No. 2 and No. 3 with a jumper wire.

1. Turn the ignition switch ON (II).

1. Check the IMRC VALVE POSITION SENSOR in the DATA LIST with the HDS.

Is about 4.90 V or higher indicated?

YES | - | Go to Step 8 .
NO | - | Go to Step 19 .