1. Check for continuity between LKAS control unit 26P connector terminal No. 24 and LKAS camera 10P connector terminal No. 3.

Is there continuity?

YES | - | Check for loose terminals in the LKAS camera and LKAS control unit connectors, and repair if necessary. If no poor connections are found, replace the LKAS camera and LKAS control unit as a set.■
NO | - | Repair an open in the wire between LKAS camera and LKAS control unit.■