Special Tools Required Sub hanger stay 07MAK-PY30100 Engine tilt hanger set 07KAK-SJ40101
Engine hanger stay
07KAK-SJ40200

1. Install the accessory brackets and tighten their bolts to the specified torques.

1. Install the engine/transmission assembly into position in the vehicle, then remove the engine tilt hanger set from the engine.
   Reinstall the mounting bolts/support nuts in the sequence given. Failure to follow this sequence may cause excessive noise and vibration, and reduce bushing life.