NOTE:

- Once you remove the door outer molding, replace it with a new one because it will bend during removal.
- Put on gloves to protect your hands.
- Take care not to scratch the door.
- When prying components, use the handy remover set or equivalent.

1. Remove the screws fastening the rear of the door weatherstrip (A), sash, and the door outer molding (B).

1. Pry the front clip with a flat-tip screwdriver.