Combination Light Switch Test/Replacement

LHD type

1. Remove the dashboard lower cover.

1. Remove the steering column covers.

1. Disconnect the 12P connector (A) from the wiper/washer switch (B).

1. Remove the two screws, then slide out the combination light switch (A).

1. Inspect the connector terminals to be sure they are all making good contact.
   - If the terminals are bent, loose or corroded, repair them as necessary, and recheck the system.
   - If the terminals look OK, check for continuity between the terminals in each switch position according to the tables.

   - | If there is no continuity replace switch.