Countershaft

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Countershaft | Diameter of needle bearing contact area (clutch housing side) | GZT5 | 40.000−40.015 mm (1.5748−1.5754 in.) | 39.95 mm (1.573 in.)
GYL3 | 35.000−35.015 mm (1.3779−1.3785 in.) | 34.95 mm (1.376 in.)
Diameter of distance collar contact area |  | 39.937−39.950 mm (1.5723−1.5728 in.) | 39.883 mm (1.5702 in.)
Diameter of ball bearing contact area (transmission housing side) |  | 30.020−30.033 mm (1.1819−1.1824 in.) | 29.97 mm (1.180 in.)
Runout |  | 0.02 mm (0.001 in.) max. | 0.05 mm (0.002 in.)
35 mm shim-to-bearing inner race clearance |  | 0.04−0.10 mm (0.0016−0.0039 in.) | Adjust