
†---------------------†

Disassembly view:

†---------------------†

  Ctrl + G             Goto
  Ctrl + E             Edit Breakpoint
  Ctrl + D             Enable/disable breakpoint
  Ctrl + B             Add breakpoint
  Left                 Go back one branch level/goto pc
  Right                Follow branch/position memory view to accessed address
  Up                   Move cursor up one line
  Down                 Move cursor down one line
  Page Up              Move visible area up one page
  Page Down            Move visible area down one page
  F10                  Step over
  F11                  Step into
  Tab                  Toggle display symbols
  Left Click           Select line/toggle breakpoint if line is already highlighted
  Right Click          Open context menu

†---------------------†

Memory View:

†---------------------†

  Ctrl + G             Goto
  Ctrl + B             Add breakpoint
  Left                 Move cursor back one byte/nibble
  Right                Move cursor ahead one byte/nibble
  Up                   Move cursor up one line
  Down                 Move cursor down one line
  Page Up              Move cursor up one page
  Page Down            Move cursor down one page
  0-9,A-F              Overwrite hex nibble
  Any                  Overwrite ansi byte
  Left Click           Select byte/nibble
  Right Click          Open context menu
  Ctrl+Wheel           Zoom memory view
  Esc                  Return to previous goto address
  Ctrl+V               Paste a hex string into memory

†---------------------†

Breakpoint List:

†---------------------†

    Up                Select previous item
    Down              Select next item
    Delete            Remove selected breakpoint
    Return            Edit selected breakpoint
    Space             Toggle enable state of selected breakpoint

†---------------------†
