Interface Statistics

                           Received            Sent

Bytes                    1030661895       202093785
Unicast packets              904390          535470
Non-unicast packets           10605            4410
Discards                          0               0
Errors                            0               0
Unknown protocols                 0

    Interface Index        = 1
    Description            = Software Loopback Interface 1
    Type                   = 24
    Mtu                    = 1500
    Speed                  = 1073741824
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 2
    Description            = WAN Miniport (PPTP)
    Type                   = 131
    Mtu                    = 1464
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 3
    Description            = Microsoft 6to4 Adapter
    Type                   = 131
    Mtu                    = 0
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 2
    Operational Status     = 6
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 4
    Description            = WAN Miniport (IKEv2)
    Type                   = 131
    Mtu                    = 1480
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 5
    Description            = Realtek Gaming 2.5GbE Family Controller
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 1000000000
    Physical Address       = 10-FF-E0-3E-94-6D
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 6
    Description            = WAN Miniport (IP)
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 7
    Description            = Microsoft IP-HTTPS Platform Adapter
    Type                   = 131
    Mtu                    = 0
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 2
    Operational Status     = 6
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 8
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #2
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = EA-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 9
    Description            = Microsoft Kernel Debug Network Adapter
    Type                   = 6
    Mtu                    = 0
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 2
    Operational Status     = 6
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 10
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = E8-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 11
    Description            = Bluetooth Device (Personal Area Network)
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 3000000
    Physical Address       = E8-47-3A-E6-2D-08
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 12
    Description            = Microsoft Teredo Tunneling Adapter
    Type                   = 131
    Mtu                    = 0
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 2
    Operational Status     = 6
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 13
    Description            = WAN Miniport (Network Monitor)
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 14
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #3
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = EE-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 15
    Description            = WAN Miniport (PPPOE)
    Type                   = 23
    Mtu                    = 1494
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 16
    Description            = WAN Miniport (SSTP)
    Type                   = 131
    Mtu                    = 4091
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 17
    Description            = WAN Miniport (L2TP)
    Type                   = 131
    Mtu                    = 1460
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 18
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #4
    Type                   = 71
    Mtu                    = 0
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 2
    Operational Status     = 6
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 19
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #5
    Type                   = 71
    Mtu                    = 0
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 2
    Operational Status     = 6
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 20
    Description            = WAN Miniport (IPv6)
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 21
    Description            = Realtek Gaming 2.5GbE Family Controller-WFP Native MAC Layer LightWeight Filter-0000
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 1000000000
    Physical Address       = 10-FF-E0-3E-94-6D
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 22
    Description            = Realtek Gaming 2.5GbE Family Controller-Realtek NDIS LightWeight Filter (NDIS 6.40)-0000
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 1000000000
    Physical Address       = 10-FF-E0-3E-94-6D
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 23
    Description            = Realtek Gaming 2.5GbE Family Controller-QoS Packet Scheduler-0000
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 1000000000
    Physical Address       = 10-FF-E0-3E-94-6D
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 24
    Description            = Realtek Gaming 2.5GbE Family Controller-WFP 802.3 MAC Layer LightWeight Filter-0000
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 1000000000
    Physical Address       = 10-FF-E0-3E-94-6D
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 25
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC-WFP Native MAC Layer LightWeight Filter-0000
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = E8-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 26
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC-Native WiFi Filter Driver-0000
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = E8-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 27
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC-Realtek NDIS LightWeight Filter (NDIS 6.40)-0000
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = E8-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 28
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC-QoS Packet Scheduler-0000
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = E8-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 29
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC-WFP 802.3 MAC Layer LightWeight Filter-0000
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = E8-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 30
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #2-WFP Native MAC Layer LightWeight Filter-0000
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = EA-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 31
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #2-Native WiFi Filter Driver-0000
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = EA-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 32
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #2-Realtek NDIS LightWeight Filter (NDIS 6.40)-0000
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = EA-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 33
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #2-QoS Packet Scheduler-0000
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = EA-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 34
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #2-WFP 802.3 MAC Layer LightWeight Filter-0000
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = EA-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 35
    Description            = WAN Miniport (IP)-WFP Native MAC Layer LightWeight Filter-0000
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 36
    Description            = WAN Miniport (IP)-Realtek NDIS LightWeight Filter (NDIS 6.40)-0000
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 37
    Description            = WAN Miniport (IP)-QoS Packet Scheduler-0000
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 38
    Description            = WAN Miniport (IPv6)-WFP Native MAC Layer LightWeight Filter-0000
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 39
    Description            = WAN Miniport (IPv6)-Realtek NDIS LightWeight Filter (NDIS 6.40)-0000
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 40
    Description            = WAN Miniport (IPv6)-QoS Packet Scheduler-0000
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 41
    Description            = WAN Miniport (Network Monitor)-WFP Native MAC Layer LightWeight Filter-0000
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 42
    Description            = WAN Miniport (Network Monitor)-Realtek NDIS LightWeight Filter (NDIS 6.40)-0000
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 43
    Description            = WAN Miniport (Network Monitor)-QoS Packet Scheduler-0000
    Type                   = 6
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = 00-00-00-00-00-00
    Administrative Status  = 1
    Operational Status     = 1
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 44
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #3-WFP Native MAC Layer LightWeight Filter-0000
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = EE-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 45
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #3-Native WiFi Filter Driver-0000
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = EE-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 46
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #3-Realtek NDIS LightWeight Filter (NDIS 6.40)-0000
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = EE-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 47
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #3-QoS Packet Scheduler-0000
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = EE-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0

    Interface Index        = 48
    Description            = Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #3-WFP 802.3 MAC Layer LightWeight Filter-0000
    Type                   = 71
    Mtu                    = 1500
    Speed                  = 0
    Physical Address       = EE-47-3A-E6-2E-84
    Administrative Status  = 1
    Operational Status     = 2
    Last Changed           = 0
    Output Queue Length    = 0
===========================================================================
Interface List
  5...10 ff e0 3e 94 6d ......Realtek Gaming 2.5GbE Family Controller
 10...e8 47 3a e6 2e 84 ......Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC
  8...ea 47 3a e6 2e 84 ......Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #2
 14...ee 47 3a e6 2e 84 ......Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC #3
 11...e8 47 3a e6 2d 08 ......Bluetooth Device (Personal Area Network)
  1...........................Software Loopback Interface 1
===========================================================================

IPv4 Route Table
===========================================================================
Active Routes:
Network Destination        Netmask          Gateway       Interface  Metric
          0.0.0.0          0.0.0.0      192.168.1.1    192.168.1.133     25
        127.0.0.0        255.0.0.0         On-link         127.0.0.1    331
        127.0.0.1  255.255.255.255         On-link         127.0.0.1    331
  127.255.255.255  255.255.255.255         On-link         127.0.0.1    331
      192.168.1.0    255.255.255.0         On-link     192.168.1.133    281
    192.168.1.133  255.255.255.255         On-link     192.168.1.133    281
    192.168.1.255  255.255.255.255         On-link     192.168.1.133    281
        224.0.0.0        240.0.0.0         On-link         127.0.0.1    331
        224.0.0.0        240.0.0.0         On-link     192.168.1.133    281
  255.255.255.255  255.255.255.255         On-link         127.0.0.1    331
  255.255.255.255  255.255.255.255         On-link     192.168.1.133    281
===========================================================================
Persistent Routes:
  None

IPv6 Route Table
===========================================================================
Active Routes:
 If Metric Network Destination      Gateway
  5     41 ::/0                     fe80::8ade:7cff:fea8:fd9a
  1    331 ::1/128                  On-link
  5     41 2603:7000:8400:1b92::/64 On-link
  5    281 2603:7000:8400:1b92::/64 fe80::8ade:7cff:fea8:fd9a
  5    281 2603:7000:8400:1b92::1569/128
                                    On-link
  5    281 2603:7000:8400:1b92:45d3:5627:cab2:ed15/128
                                    On-link
  5    281 2603:7000:8400:1b92:f911:e1e7:5092:9bee/128
                                    On-link
  5     41 fd00:88de:7ca8:fd9a::/64 On-link
  5    281 fd00:88de:7ca8:fd9a:6250:7d1b:3dfa:f2b6/128
                                    On-link
  5    281 fd00:88de:7ca8:fd9a:f911:e1e7:5092:9bee/128
                                    On-link
  5    281 fe80::/64                On-link
  5    281 fe80::e309:d40e:dfcb:df0/128
                                    On-link
  1    331 ff00::/8                 On-link
  5    281 ff00::/8                 On-link
===========================================================================
Persistent Routes:
  None

Active Connections

  Proto  Local Address          Foreign Address        State           PID
  TCP    0.0.0.0:135            Peter:0                LISTENING       1564
  RpcEptMapper
 [System]
  TCP    0.0.0.0:445            Peter:0                LISTENING       4
 Can not obtain ownership information
  TCP    0.0.0.0:5040           Peter:0                LISTENING       8028
  CDPSvc
 [System]
  TCP    0.0.0.0:5985           Peter:0                LISTENING       4
 Can not obtain ownership information
  TCP    0.0.0.0:7680           Peter:0                LISTENING       4784
 Can not obtain ownership information
  TCP    0.0.0.0:27036          Peter:0                LISTENING       9652
 [steam.exe]
  TCP    0.0.0.0:47001          Peter:0                LISTENING       4
 Can not obtain ownership information
  TCP    0.0.0.0:49664          Peter:0                LISTENING       1236
 Can not obtain ownership information
  TCP    0.0.0.0:49665          Peter:0                LISTENING       1136
 Can not obtain ownership information
  TCP    0.0.0.0:49666          Peter:0                LISTENING       2124
  Schedule
 [System]
  TCP    0.0.0.0:49667          Peter:0                LISTENING       2452
  EventLog
 [System]
  TCP    0.0.0.0:49668          Peter:0                LISTENING       2096
  Spooler
 [System]
  TCP    0.0.0.0:49697          Peter:0                LISTENING       1208
 Can not obtain ownership information
  TCP    127.0.0.1:27060        Peter:0                LISTENING       9652
 [steam.exe]
  TCP    127.0.0.1:49755        Peter:0                LISTENING       9652
 [steam.exe]
  TCP    127.0.0.1:49755        Peter:49767            ESTABLISHED     9652
 [steam.exe]
  TCP    127.0.0.1:49756        Peter:0                LISTENING       9652
 [steam.exe]
  TCP    127.0.0.1:49756        Peter:49766            ESTABLISHED     9652
 [steam.exe]
  TCP    127.0.0.1:49766        Peter:49756            ESTABLISHED     11128
 [System]
  TCP    127.0.0.1:49767        Peter:49755            ESTABLISHED     11128
 [System]
  TCP    192.168.1.133:139      Peter:0                LISTENING       4
 Can not obtain ownership information
  TCP    192.168.1.133:50272    lga34s33-in-f14.1e100.net:https  TIME_WAIT       0
  TCP    192.168.1.133:50279    169-150-236-105.bunnyinfra.net:https  TIME_WAIT       0
  TCP    192.168.1.133:50283    a23-200-0-186.deploy.static.akamaitechnologies.com:http  TIME_WAIT       0
  TCP    192.168.1.133:50287    162-254-192-98.valve.net:https  TIME_WAIT       0
  TCP    192.168.1.133:50288    162-254-192-99.valve.net:27019  TIME_WAIT       0
  TCP    192.168.1.133:50289    162-254-192-99.valve.net:27018  TIME_WAIT       0
  TCP    192.168.1.133:50290    162-254-193-103.valve.net:27019  ESTABLISHED     9652
 [steam.exe]
  TCP    192.168.1.133:50291    40.69.76.172:https     TIME_WAIT       0
  TCP    192.168.1.133:50311    20.189.173.4:https     TIME_WAIT       0
  TCP    192.168.1.133:50313    172.183.7.194:https    ESTABLISHED     5688
  WpnService
 [System]
  TCP    192.168.1.133:50314    104.20.184.56:https    TIME_WAIT       0
  TCP    192.168.1.133:50317    104.26.12.6:https      TIME_WAIT       0
  TCP    192.168.1.133:50324    172.178.160.20:https   ESTABLISHED     5700
 Can not obtain ownership information
  TCP    192.168.1.133:50326    a-0003.a-msedge.net:https  TIME_WAIT       0
  TCP    192.168.1.133:50327    a-0003.a-msedge.net:https  ESTABLISHED     9340
 [System]
  TCP    192.168.1.133:50338    40.118.171.167:https   ESTABLISHED     9500
 [System]
  TCP    192.168.1.133:50339    172.183.192.109:https  ESTABLISHED     9500
 [System]
  TCP    192.168.1.133:50340    249.195.120.34.bc.googleusercontent.com:https  ESTABLISHED     2752
 [SysnativeFileCollectionApp.exe]
  TCP    [::]:135               Peter:0                LISTENING       1564
  RpcEptMapper
 [System]
  TCP    [::]:445               Peter:0                LISTENING       4
 Can not obtain ownership information
  TCP    [::]:5985              Peter:0                LISTENING       4
 Can not obtain ownership information
  TCP    [::]:7680              Peter:0                LISTENING       4784
 Can not obtain ownership information
  TCP    [::]:47001             Peter:0                LISTENING       4
 Can not obtain ownership information
  TCP    [::]:49664             Peter:0                LISTENING       1236
 Can not obtain ownership information
  TCP    [::]:49665             Peter:0                LISTENING       1136
 Can not obtain ownership information
  TCP    [::]:49666             Peter:0                LISTENING       2124
  Schedule
 [System]
  TCP    [::]:49667             Peter:0                LISTENING       2452
  EventLog
 [System]
  TCP    [::]:49668             Peter:0                LISTENING       2096
  Spooler
 [System]
  TCP    [::]:49697             Peter:0                LISTENING       1208
 Can not obtain ownership information
  TCP    [::1]:50341            Peter:5985             TIME_WAIT       0
  TCP    [::1]:50342            Peter:5985             TIME_WAIT       0
  TCP    [::1]:50343            Peter:5985             TIME_WAIT       0
  TCP    [::1]:50344            Peter:5985             TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50297  lga34s35-in-x05.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50298  lga34s32-in-x05.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50299  lga34s30-in-x0e.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50300  lga25s74-in-x03.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50301  lga34s38-in-x0a.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50302  lga34s32-in-x0a.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50303  lga34s31-in-x0e.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50304  lga34s36-in-x03.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50305  lga25s73-in-x0a.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50306  lga34s35-in-x0a.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50307  lga25s79-in-x0a.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50308  lga34s31-in-x0a.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50310  lga25s79-in-x11.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50312  lga34s38-in-x0e.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50318  lga25s80-in-x0e.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50320  lga34s39-in-x0a.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50321  lga34s31-in-x0a.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50323  lga15s46-in-x0e.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50325  g2600-1400-9000-0000-0000-0000-6875-b643.deploy.static.akamaitechnologies.com:https  ESTABLISHED     9340
 [System]
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50329  [2a04:4e42:56::684]:http  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50330  lga25s41-in-x03.1e100.net:http  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50331  g2600-1400-b000-048e-0000-0000-0000-21cc.deploy.static.akamaitechnologies.com:http  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50333  [2a04:4e42:56::684]:http  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50335  lga34s30-in-x05.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50336  lga25s81-in-x05.1e100.net:https  TIME_WAIT       0
  TCP    [2603:7000:8400:1b92:f911:e1e7:5092:9bee]:50337  pe-in-f188.1e100.net:5228  ESTABLISHED     5684
 [System]
  UDP    0.0.0.0:5050           *:*                                    8028
  CDPSvc
 [System]
  UDP    0.0.0.0:5353           *:*                                    16280
 [System]
  UDP    0.0.0.0:5353           *:*                                    2824
  Dnscache
 [System]
  UDP    0.0.0.0:5353           *:*                                    16280
 [System]
  UDP    0.0.0.0:5355           *:*                                    2824
  Dnscache
 [System]
  UDP    0.0.0.0:9527           *:*                                    7424
 [System]
  UDP    0.0.0.0:27036          *:*                                    9652
 [steam.exe]
  UDP    0.0.0.0:49481          0.0.32.14:443                          5684
 [System]
  UDP    0.0.0.0:49620          0.0.0.84:443                           5684
 [System]
  UDP    0.0.0.0:49943          0.0.32.3:443                           5684
 [System]
  UDP    0.0.0.0:53968          0.0.32.14:443                          5684
 [System]
  UDP    0.0.0.0:54141          0.0.32.14:443                          5684
 [System]
  UDP    0.0.0.0:54376          *:*                                    2824
  Dnscache
 [System]
  UDP    0.0.0.0:54460          0.0.32.3:443                           5684
 [System]
  UDP    0.0.0.0:55396          142.250.80.42:443                      5684
 [System]
  UDP    0.0.0.0:60925          *:*                                    2824
  Dnscache
 [System]
  UDP    0.0.0.0:65369          142.251.35.170:443                     5684
 [System]
  UDP    127.0.0.1:49296        127.0.0.1:49296                        5196
  iphlpsvc
 [System]
  UDP    192.168.1.133:137      *:*                                    4
 Can not obtain ownership information
  UDP    192.168.1.133:138      *:*                                    4
 Can not obtain ownership information
  UDP    192.168.1.133:27036    *:*                                    9652
 [steam.exe]
  UDP    [::]:5353              *:*                                    16280
 [System]
  UDP    [::]:5353              *:*                                    2824
  Dnscache
 [System]
  UDP    [::]:5355              *:*                                    2824
  Dnscache
 [System]
  UDP    [::]:49481             [2607:f8b0:4006:80c::200e]:443                  5684
 [System]
  UDP    [::]:49620             [2607:f8b0:4004:c19::54]:443                  5684
 [System]
  UDP    [::]:49943             [2607:f8b0:4006:820::2003]:443                  5684
 [System]
  UDP    [::]:53968             [2607:f8b0:4006:80d::200e]:443                  5684
 [System]
  UDP    [::]:54141             [2607:f8b0:4006:806::200e]:443                  5684
 [System]
  UDP    [::]:54376             *:*                                    2824
  Dnscache
 [System]
  UDP    [::]:54460             [2607:f8b0:4006:820::2003]:443                  5684
 [System]
  UDP    [::]:60925             *:*                                    2824
  Dnscache
 [System]
