Wireless System Information Summary
(Time: 5/24/2025 7:03:17 PM Eastern Daylight Time)


======================================================================= 
============================== SHOW DRIVERS =========================== 
=======================================================================


Interface name: Wi-Fi

    Driver                    : Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC
    Vendor                    : Realtek Semiconductor Corp.
    Provider                  : Realtek Semiconductor Corp.
    Date                      : 11/27/2024
    Version                   : 6101.19.126.0
    INF file                  : oem44.inf
    Type                      : Native Wi-Fi Driver
    Radio types supported     : 802.11b 802.11g 802.11n 802.11ac 802.11ax 802.11a
    FIPS 140 mode supported   : Yes
    802.11w Management Frame Protection supported : Yes
    Hosted network supported  : No
    Authentication and cipher supported in infrastructure mode:
                                Open             None
                                WPA2-Personal    CCMP
                                Open             WEP-40bit
                                Open             WEP-104bit
                                Open             WEP
                                WPA-Enterprise   TKIP
                                WPA-Personal     TKIP
                                WPA2-Enterprise  TKIP
                                WPA2-Personal    TKIP
                                WPA-Enterprise   CCMP
                                WPA-Personal     CCMP
                                WPA2-Enterprise  CCMP
                                WPA3-Personal    CCMP
                                WPA3-Enterprise 192 Bits GCMP-256
                                OWE              CCMP
                                Vendor defined   TKIP
                                Vendor defined   CCMP
                                Vendor defined   Vendor defined
                                Vendor defined   Vendor defined
                                WPA2-Enterprise  Vendor defined
                                WPA2-Enterprise  Vendor defined
                                Vendor defined   Vendor defined
                                Vendor defined   Vendor defined
                                WPA3-Enterprise  CCMP
    Number of supported bands : 2
                                2.4 GHz [ 2412 MHz - 2484 MHz]
                                5 GHz [ 5180 MHz - 5885 MHz]
    Wireless Display Supported: Yes (Graphics Driver: Yes, Wi-Fi Driver: Yes)


======================================================================= 
============================= SHOW INTERFACES ========================= 
=======================================================================


There is 1 interface on the system: 

    Name                   : Wi-Fi
    Description            : Realtek 8851BE Wireless LAN WiFi 6 PCI-E NIC
    GUID                   : 8136d4f8-d6c6-4c6e-91ca-35351b9f3815
    Physical address       : e8:47:3a:e6:2e:84
    Interface type         : Primary
    State                  : disconnected
    Radio status           : Hardware On
                             Software On

    Hosted network status  : Not available


======================================================================= 
=========================== SHOW HOSTED NETWORK ======================= 
=======================================================================


Hosted network settings 
----------------------- 
    Mode                   : Allowed
    Settings               : <Not configured>

Hosted network status 
--------------------- 
    Status                 : Not available


======================================================================= 
============================= SHOW SETTINGS =========================== 
=======================================================================


Wireless LAN settings 
--------------------- 
    Show blocked networks in visible network list: No

    Only use GP profiles on GP-configured networks: No

    Hosted network mode allowed in WLAN service: Yes

    Allow shared user credentials for network authentication: Yes

    Block period: Not Configured.

    Auto configuration logic is enabled on interface "Wi-Fi"
    MAC randomization disabled on interface Wi-Fi


======================================================================= 
============================== SHOW FILTERS =========================== 
=======================================================================


Allow list on the system (group policy) 
--------------------------------------- 
    <None>

Allow list on the system (user) 
------------------------------- 
    <None>

Block list on the system (group policy) 
--------------------------------------- 
    <None>

Block list on the system (user) 
------------------------------- 
    <None>


======================================================================= 
=========================== SHOW CREATEALLUSER ======================== 
=======================================================================


Everyone is allowed to create all user profiles.


======================================================================= 
============================= SHOW PROFILES =========================== 
=======================================================================


Profiles on interface Wi-Fi:

Group policy profiles (read only)
---------------------------------
    <None>

User profiles
-------------
    All User Profile     : Peter’s iPhone
    All User Profile     : SpectrumSetup-99
    All User Profile     : MySpectrumWiFice-5G


======================================================================= 
========================== SHOW PROFILES NAMES ======================== 
=======================================================================


Profile Peter’s iPhone on interface Wi-Fi: 
======================================================================= 

Applied: All User Profile    

Profile information 
------------------- 
    Version                : 1
    Type                   : Wireless LAN
    Name                   : Peter’s iPhone
    Control options        : 
        Connection mode    : Connect automatically
        Network broadcast  : Connect only if this network is broadcasting
        AutoSwitch         : Do not switch to other networks
        MAC Randomization  : Disabled

Connectivity settings 
--------------------- 
    Number of SSIDs        : 1
    SSID name              : "Peter’s iPhone"
    Network type           : Infrastructure
    Radio type             : [ Any Radio Type ]
    Vendor extension          : Not present

Security settings 
----------------- 
    Authentication         : WPA3-Personal
    Cipher                 : GCMP-256
    Authentication         : WPA3-Personal
    Cipher                 : GCMP
    Authentication         : WPA3-Personal
    Cipher                 : CCMP
    Security key           : Present

Cost settings 
------------- 
    Cost                   : Unrestricted
    Congested              : No
    Approaching Data Limit : No
    Over Data Limit        : No
    Roaming                : No
    Cost Source            : Default


Profile SpectrumSetup-99 on interface Wi-Fi: 
======================================================================= 

Applied: All User Profile    

Profile information 
------------------- 
    Version                : 1
    Type                   : Wireless LAN
    Name                   : SpectrumSetup-99
    Control options        : 
        Connection mode    : Connect manually
        Network broadcast  : Connect only if this network is broadcasting
        AutoSwitch         : Do not switch to other networks
        MAC Randomization  : Disabled

Connectivity settings 
--------------------- 
    Number of SSIDs        : 1
    SSID name              : "SpectrumSetup-99"
    Network type           : Infrastructure
    Radio type             : [ Any Radio Type ]
    Vendor extension          : Not present

Security settings 
----------------- 
    Authentication         : WPA3-Personal
    Cipher                 : GCMP-256
    Authentication         : WPA3-Personal
    Cipher                 : GCMP
    Authentication         : WPA3-Personal
    Cipher                 : CCMP
    Authentication         : WPA2-Personal
    Cipher                 : GCMP
    Authentication         : WPA2-Personal
    Cipher                 : CCMP
    Security key           : Present

Cost settings 
------------- 
    Cost                   : Unrestricted
    Congested              : No
    Approaching Data Limit : No
    Over Data Limit        : No
    Roaming                : No
    Cost Source            : Default


Profile MySpectrumWiFice-5G on interface Wi-Fi: 
======================================================================= 

Applied: All User Profile    

Profile information 
------------------- 
    Version                : 1
    Type                   : Wireless LAN
    Name                   : MySpectrumWiFice-5G
    Control options        : 
        Connection mode    : Connect manually
        Network broadcast  : Connect only if this network is broadcasting
        AutoSwitch         : Do not switch to other networks
        MAC Randomization  : Disabled

Connectivity settings 
--------------------- 
    Number of SSIDs        : 1
    SSID name              : "MySpectrumWiFice-5G"
    Network type           : Infrastructure
    Radio type             : [ Any Radio Type ]
    Vendor extension          : Not present

Security settings 
----------------- 
    Authentication         : WPA2-Personal
    Cipher                 : GCMP
    Authentication         : WPA2-Personal
    Cipher                 : CCMP
    Security key           : Present

Cost settings 
------------- 
    Cost                   : Unrestricted
    Congested              : No
    Approaching Data Limit : No
    Over Data Limit        : No
    Roaming                : No
    Cost Source            : Default


======================================================================= 
======================= SHOW NETWORKS MODE=BSSID ====================== 
=======================================================================

 
Interface name : Wi-Fi 
There are 9 networks currently visible. 

SSID 1 : Verizon_NWF7PZ
    Network type            : Infrastructure
    Authentication          : WPA2-Personal
    Encryption              : CCMP 
    BSSID 1                 : dc:f5:1b:66:d4:11
         Signal             : 12%  
         Radio type         : 802.11n
         Band               : 2.4 GHz
         Channel            : 11 
         Bss Load:
             Connected Stations:         0
             Channel Utilization:        139 (54 %)
             Medium Available Capacity:  0 (0 us/s)
         QoS MSCS Supported    : 0
         QoS Map Supported     : 1
         Basic rates (Mbps) : 1 2 5.5 11
         Other rates (Mbps) : 6 9 12 18 24 36 48 54
    BSSID 2                 : 8a:f5:1b:66:d4:15
         Signal             : 5%  
         Radio type         : 802.11ax
         Band               : 5 GHz
         Channel            : 60 
         Bss Load:
             Connected Stations:         0
             Channel Utilization:        8 (3 %)
             Medium Available Capacity:  0 (0 us/s)
         QoS MSCS Supported    : 0
         QoS Map Supported     : 0
         Basic rates (Mbps) : 6 12 24
         Other rates (Mbps) : 9 18 36 48 54
    BSSID 3                 : 82:f5:1b:66:d4:14
         Signal             : 14%  
         Radio type         : 802.11ax
         Band               : 5 GHz
         Channel            : 116 
         Bss Load:
             Connected Stations:         0
             Channel Utilization:        5 (1 %)
             Medium Available Capacity:  0 (0 us/s)
         QoS MSCS Supported    : 0
         QoS Map Supported     : 0
         Basic rates (Mbps) : 6 12 24
         Other rates (Mbps) : 9 18 36 48 54

SSID 2 : Verizon_JX6SQP
    Network type            : Infrastructure
    Authentication          : WPA2-Personal
    Encryption              : CCMP 
    BSSID 1                 : 24:41:fe:65:bc:8b
         Signal             : 13%  
         Radio type         : 802.11n
         Band               : 2.4 GHz
         Channel            : 6 
         QoS MSCS Supported    : 0
         QoS Map Supported     : 0
         Basic rates (Mbps) : 1 2 5.5 11
         Other rates (Mbps) : 6 9 12 18 24 36 48 54
    BSSID 2                 : 24:41:fe:65:bc:8c
         Signal             : 10%  
         Radio type         : 802.11ax
         Band               : 5 GHz
         Channel            : 48 
         QoS MSCS Supported    : 0
         QoS Map Supported     : 0
         Basic rates (Mbps) : 6 12 24
         Other rates (Mbps) : 9 18 36 48 54

SSID 3 : bd-office
    Network type            : Infrastructure
    Authentication          : WPA2-Personal
    Encryption              : CCMP 
    BSSID 1                 : b0:2a:43:e0:1a:5c
         Signal             : 10%  
         Radio type         : 802.11n
         Band               : 2.4 GHz
         Channel            : 6 
         QoS MSCS Supported    : 0
         QoS Map Supported     : 0
         Basic rates (Mbps) : 1 2 5.5 11
         Other rates (Mbps) : 6 9 12 18 24 36 48 54
    BSSID 2                 : b0:2a:43:e0:1a:58
         Signal             : 12%  
         Radio type         : 802.11ac
         Band               : 5 GHz
         Channel            : 149 
         QoS MSCS Supported    : 0
         QoS Map Supported     : 0
         Basic rates (Mbps) : 6 12 24
         Other rates (Mbps) : 9 18 36 48 54
    BSSID 3                 : 30:fd:38:f6:46:61
         Signal             : 2%  
         Radio type         : 802.11n
         Band               : 2.4 GHz
         Channel            : 6 
         QoS MSCS Supported    : 0
         QoS Map Supported     : 0
         Basic rates (Mbps) : 1 2 5.5 11
         Other rates (Mbps) : 6 9 12 18 24 36 48 54

SSID 4 : TMOF013
    Network type            : Infrastructure
    Authentication          : WPA3-Personal
    Encryption              : CCMP 
    BSSID 1                 : 64:67:72:62:f0:16
         Signal             : 5%  
         Radio type         : 802.11ax
         Band               : 5 GHz
         Channel            : 149 
         Details            :  (H2E Not supported) 
         Bss Load:
             Connected Stations:         2
             Channel Utilization:        11 (4 %)
             Medium Available Capacity:  0 (0 us/s)
         QoS MSCS Supported    : 0
         QoS Map Supported     : 1
         Basic rates (Mbps) : 6 12 24
         Other rates (Mbps) : 9 18 36 48 54

SSID 5 : Fios-IL2YZ-5G
    Network type            : Infrastructure
    Authentication          : WPA2-Personal
    Encryption              : CCMP 
    BSSID 1                 : 20:c0:47:d6:41:8e
         Signal             : 9%  
         Radio type         : 802.11ac
         Band               : 5 GHz
         Channel            : 36 
         Bss Load:
             Connected Stations:         2
             Channel Utilization:        33 (12 %)
             Medium Available Capacity:  0 (0 us/s)
         QoS MSCS Supported    : 0
         QoS Map Supported     : 0
         Basic rates (Mbps) : 6 12 24
         Other rates (Mbps) : 9 18 36 48 54

SSID 6 : Spectrum Mobile
    Network type            : Infrastructure
    Authentication          : WPA2-Enterprise
    Encryption              : CCMP 
    BSSID 1                 : 6a:de:7c:a8:fd:98
         Signal             : 10%  
         Radio type         : 802.11ax
         Band               : 5 GHz
         Channel            : 44 
         QoS MSCS Supported    : 0
         QoS Map Supported     : 0
         Basic rates (Mbps) : 6 12 24
         Other rates (Mbps) : 9 18 36 48 54

SSID 7 : 
    Network type            : Infrastructure
    Authentication          : WPA2-Personal
    Encryption              : CCMP 
    BSSID 1                 : 8a:f5:1b:66:d4:14
         Signal             : 5%  
         Radio type         : 802.11ax
         Band               : 5 GHz
         Channel            : 60 
         Bss Load:
             Connected Stations:         0
             Channel Utilization:        8 (3 %)
             Medium Available Capacity:  0 (0 us/s)
         QoS MSCS Supported    : 0
         QoS Map Supported     : 0
         Basic rates (Mbps) : 6 12 24
         Other rates (Mbps) : 9 18 36 48 54
    BSSID 2                 : 82:f5:1b:66:d4:13
         Signal             : 13%  
         Radio type         : 802.11ax
         Band               : 5 GHz
         Channel            : 116 
         Bss Load:
             Connected Stations:         0
             Channel Utilization:        5 (1 %)
             Medium Available Capacity:  0 (0 us/s)
         QoS MSCS Supported    : 0
         QoS Map Supported     : 0
         Basic rates (Mbps) : 6 12 24
         Other rates (Mbps) : 9 18 36 48 54
    BSSID 3                 : 22:c0:47:d6:41:8f
         Signal             : 9%  
         Radio type         : 802.11ac
         Band               : 5 GHz
         Channel            : 36 
         Bss Load:
             Connected Stations:         0
             Channel Utilization:        36 (14 %)
             Medium Available Capacity:  0 (0 us/s)
         QoS MSCS Supported    : 0
         QoS Map Supported     : 0
         Basic rates (Mbps) : 6 12 24
         Other rates (Mbps) : 9 18 36 48 54

SSID 8 : Fios-IL2YZ_Ext
    Network type            : Infrastructure
    Authentication          : WPA2-Personal
    Encryption              : CCMP 
    BSSID 1                 : e8:9f:80:12:a5:a0
         Signal             : 7%  
         Radio type         : 802.11n
         Band               : 2.4 GHz
         Channel            : 11 
         QoS MSCS Supported    : 0
         QoS Map Supported     : 0
         Basic rates (Mbps) : 1 2 5.5 11
         Other rates (Mbps) : 6 9 12 18 24 36 48 54

SSID 9 : SpectrumSetup-99
    Network type            : Infrastructure
    Authentication          : WPA2-Personal
    Encryption              : CCMP 
    BSSID 1                 : 88:de:7c:a8:fd:97
         Signal             : 14%  
         Radio type         : 802.11ax
         Band               : 2.4 GHz
         Channel            : 1 
         QoS MSCS Supported    : 0
         QoS Map Supported     : 0
         Basic rates (Mbps) : 1 2 5.5 11
         Other rates (Mbps) : 6 9 12 18 24 36 48 54
    BSSID 2                 : 88:de:7c:a8:fd:98
         Signal             : 10%  
         Radio type         : 802.11ax
         Band               : 5 GHz
         Channel            : 44 
         QoS MSCS Supported    : 0
         QoS Map Supported     : 0
         Basic rates (Mbps) : 6 12 24
         Other rates (Mbps) : 9 18 36 48 54


======================================================================= 
======================= SHOW INTERFACE CAPABILITIES =================== 
=======================================================================


Wireless System Capabilities 
---------------------------- 
    Number of antennas connected to the 802.11 radio (value not available)
    Max number of channels the device can operate on, simultaneously (value not available)
    Co-existence Support                        : Unknown


Wireless Device Capabilities 
---------------------------- 

Interface name: Wi-Fi

    WDI Version (Windows)                       : 0.2.0.12
    WDI Version (IHV)                           : 0.2.0.12
    WiFiCx Version (Windows)                    : 1.2
    WiFiCx Version (IHV)                        : 1.0
    Firmware Version                            : rtwlane
    Station                                     : Supported
    Soft AP                                     : Not supported
    Network monitor mode                        : Not supported
    Wi-Fi Direct Device                         : Supported
    Wi-Fi Direct GO                             : Supported
    Wi-Fi Direct Client                         : Supported
    Protected Management Frames                 : Supported
    DOT11k neighbor report                      : Supported
    ANQP Service Information Discovery          : Supported
    Action Frame                                : Supported
    Diversity Antenna                           : Unknown
    IBSS                                        : Not Supported
    Promiscuous Mode                            : Not Supported
    P2P Device Discovery                        : Supported
    P2P Service Name Discovery                  : Not Supported
    P2P Service Info Discovery                  : Not Supported
    P2P Background Discovery                    : Not Supported
    P2P GO on 5 GHz                             : Supported
    P2P GO on 6 GHz                             : Not Supported
    P2P Sae on GO                               : Not Supported
    ASP 2.0 Service Name Discovery              : Not Supported
    ASP 2.0 Service Information Discovery       : Not Supported
    IP Docking Capable                          : Not Supported
    Host FIPS Mode                              : Supported
    Instant Connect                             : Supported
    Dx Standby NLO                              : Supported
    Extended Channel Switch Announcement        : Supported
    Function Level Reset                        : Not Supported
    Platform Level Reset                        : Supported
    Bus Level Reset                             : Supported
    MAC Randomization                           : Supported
    Fast Transition                             : Supported
    MU-MIMO                                     : Supported
    Miracast Sink                               : Supported
    BSS Transition (802.11v)                    : Supported
    IHV Extensibility Module Configured         : Not Supported
    SAE Authentication                          : Supported
    SAE Hash-to-Element Authentication          : Supported
    WPA3 SUITE-B Authentication                 : Not Supported
    OWE Authentication                          : Supported
    FTM as Initiator                            : Not Supported
    MBO Support                                 : Supported
    Number of Tx Spatial Streams                : 1
    Number of Rx Spatial Streams                : 1
    Number of Concurrent Channels Supported     : 0
    Number of Radios                            : 0
    P2P GO ports count                          : 1
    P2P Clients Port Count                      : 1
    P2P Max Mobile AP Clients                   : 8
    Max ANQP Service Advertisements Supported   : 0
    Maximum Number of Secondary STAs Supported  : 0
    Number of MLO Connections Supported         : 0
    QoS MSCS Supported                          : Not Supported
    QoS DSCP to UP Mapping Supported            : Not Supported
    Wpa3-Sae with 384-bit Pmk Supported         : Not Supported
    Cross Akm/Cipher Roaming                    : Not Supported
    Co-existence Support                        : Wi-Fi performance is maintained



The Wired AutoConfig Service (dot3svc) is not running.


The Wired AutoConfig Service (dot3svc) is not running.


The Wired AutoConfig Service (dot3svc) is not running.

