For some models: SRS components are located in this area. Review the SRS component locations LHD, SRS component location RHD and the precautions and procedures before performing repairs or service. NOTE When prying components, use the handy remover set or equivalent. Take care not to scratch the body or tear the seat covers. Put on gloves to protect your hands. Raise the steering column all the way up, and telescope it all the way in. Slide the seat all the way forward, then remove the seat track end covers (A) from the back of both seat tracks. Slide the seat to the rear, about halfway so you can access the seat mounting bolts. If equipped with the 8-way power seat, fully raise the seat. If equipped with a side airbag, disconnect the negative battery cable, and wait at least 3 minutes before removing the seat. | Manual/manual height adjustable 4-way power/8-way power