Fuse to Components Index - Under-hood Fuse/Relay Box

Under-hood Fuse/Relay Box

Fuse Number | Amps | Wire Color | Component(s) or Circuit(s) Protected
--- | --- | --- | ---
1 | 15 A | RED/YEL | Left headlight (low beam)
2 | 30 A | ——— | Control block (relay control module)
3 | 10 A | WHT/YEL | Left headlight (high beam)
4 | 15 A | ——— | Dash lights, Front parking lights, License place lights, Relay control module, Taillights, VSA OFF switch
5 | 10 A | WHT/GRN | Right headlight (high beam)
6 | 15 A | RED/GRN | Right headlight (high beam), High beam indicator
7 | 7.5 A | ——— | Control block (relay control module)
8 | 20 A | WHT/GRN | Data link connector, ELD unit, Inertia switch, PGM-FI main relay 1 and 2, Fuel heater relay
9 | 20 A | BLU/YEL | A/C condenser fan motor
BLU/RED | A/C compressor clutch
10 | 20 A | WHT/BLK | Fuel pump
11 | 30 A | WHT/BLK | Fuel heater switch
12 | 30 A | BLK/RED | No. 1 fuse (in the multi-fuse/relay box), No. 3 and 4 fuses (in the under-dash fuse/relay box)
13 | 20 A | RED | ABS modulator-control unit, Brake lights, ECM, Horns, Horn relay, Ignition key light, Multiplex integrated control unit, VSA modulator-control unit
14 | 40 A | BLK/YEL | Antenna coil, Rear window defogger
15 | 30 A | ——— | No. 7 fuse (in the under-hood fuse/relay box)
YEL | No. 5, 6, 7, 8, and 9 fuses (in the under-dash fuse/relay box)
16 | 15 A | WHT/BLK | Hazard warning light relays, Turn signal/hazard relay
17 | 30 A | WHT/RED | ABS or VSA modulator-control unit
18 | 20 A | WHT | ABS modulator-control unit
40 A | WHT | VSA modulator-control unit
19 | 30 A | RED | Radiator fan motor
20 | 40 A | BLU | No. 13, 14, 15, 16, and 17 fuses (in the under-dash fuse/relay box)
21 | 40 A | WHT/BLU | Blower motor
22 (GLOW) | 70 A | WHT | Glow plug control module
22 (BAT) | 100 A | ——— | Battery, Power distribution
23 (IG) | 50 A | WHT | Ignition switch
23 (P/W) | 50 A | WHT/BLU | No. 24, 25, 26, 27, and 28 fuses (in the under-dash fuse/relay box), Power window relay