DTC P0107: MAP Sensor Circuit Low Voltage Turn the ignition switch ON (II). Check the MAP SENSOR in the DATA LIST with the HDS. Is about 0.2 V or less indicated?
YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the MAP/IAT sensor and the ECM.■
Turn the ignition switch OFF. Disconnect the MAP/IAT sensor 4P connector. Turn the ignition switch ON (II). Check the MAP SENSOR in the DATA LIST with the HDS. Is about 0.2 V or less indicated?
YES | - | Go to Step 12 .
NO | - | Go to Step 7 .
Measure voltage between MAP/IAT sensor 4P connector terminals No. 1 and No. 4. Is there about 5 V?
YES | - | Go to Step 15 .
NO | - | Go to Step 8 .
Turn the ignition switch OFF, and wait 30 seconds. Disconnect ECM connector No. 1 (96P). |